BPM DOCUMENTATION

Contents

[**0xDEADBEEF** 1](#_Toc531013241)

[**Purpose of document** 1](#_Toc531013242)

[**Requirements** 2](#_Toc531013243)

[POST/Power on (Harrison James Marcks) 2](#_Toc531013244)

[Sphygmomanometer (Harrison James Marcks) 3](#_Toc531013245)

[Human Interface (Huseyin Sert) 3](#_Toc531013246)

[Screen (Huseyin Sert) 4](#_Toc531013247)

[**Acceptance Tests** 5](#_Toc531013248)

[**POST/Power On (Harrison James Marcks)** 5](#_Toc531013249)

[**Blood Pressure Machine (Huseyin Sert)** 7](#_Toc531013250)

[**Human Interface (Huseyin Sert)** 8](#_Toc531013251)

[**Screen (Huseyin Sert)** 10](#_Toc531013252)

[**Designs** 13](#_Toc531013253)

[**Screen** 13](#_Toc531013254)

[High Level (Huseyin Sert) 13](#_Toc531013255)

# **0xDEADBEEF**

Members are as follows:

* Huseyin Sert (HS)
* Jesse Batt (JB)
* Harrison James Marcks (HJM)
* Dan Steer (DS)

# **Purpose of document**

This document aims to bring all documentation created for the BPM under one file.

Each member had their own components to complete for requirements, acceptance tests, high level designs and low level designs.

Note: For this submission, we have not created the low level designs (Jackson Diagrams). The reason for this is, we have not yet seen enough code or looked thoroughly through the hardware for the Blood Pressure Machine component.

On the contents page you can see a name next to each component. This mean that component is accomplished by that name. There is also the **WhoDidWhat\_Documentation\_Review\_BPM.doc** document which gives more concise and easy to follow version of individual progress along with all the reviews made by users to each other’s work.

# **Requirements**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ID | SUMMARY OF REQUIREMENT  (I WANT TO) | | RATIONALE  (SO THAT I CAN) | PRIORITY | SOURCE | CREATED |
| POST/Power on (Harrison James Marcks) | | | | | | |
| P1 | Be able to test the memory | Verify the board will work correctly | | S |  | 04/10/2018 |
| P2 | Be able to test the screen | Verify the screen will display correctly | | S |  | 04/10/2018 |
| P3 | Be able to test the CPU (Jump instructions) | Verify the board will work correctly | | S |  | 04/10/2018 |
| P4 | Be able to test the power | Verify the board will work correctly | | S |  | 04/10/2018 |
| P5 | Be able to test ROM | Verify the board will work correctly | | S |  | 04/10/2018 |
| P6 | Be able to perform POST/Power on the device | So the board can actually be used and boot up | | S |  | 04/10/2018 |
| P7 | Be able to check buttons | So that the buttons can be used | | S |  | 04/10/2018 |
| P8 | Check network interface | So that we can wired devices | | N |  | 04/10/2018 |
| P9 | Check blue tooth module | So that we can connect devices | | N |  | 04/10/2018 |
| P10 | All tests run automatically on system start | Perform the tests automatically every time it is started | | C |  | 12/11/2018 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sphygmomanometer (Harrison James Marcks) | | | | | |
| B1 | Measure a user’s blood pressure | Take readings and make medical judgements | S |  | 15/10/2018 |
| B2 | Send BP readings to screen | View a user’s blood pressure | S |  | 15/10/2018 |
| B3 | Read data from the reader | So that readings can be gathered | S |  | 17/10/2018 |
| B4 | Take average blood pressure | Have better results | C |  | 17/10/2018 |
| B5 | Filter out erroneous readings and data | Have more accurate results | S |  | 17/10/2018 |
| B6 | Measure blood pressure in real time | Read more relevant ratings | S |  | 17/10/2018 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Human Interface (Huseyin Sert) | | | | | |
| H1 | Perform a single button click | Interact with the device, select options | S |  | 25/11/2018 |
| H2 | Perform a double button click | Interact with the device, trigger secondary(subtasks) tasks | C |  | 25/11/2018 |
| H3 | Perform a long button click | Interact with the device, trigger secondary(subtasks) tasks | C |  | 25/11/2018 |
| H4 | Perform a multi-button click | Interact with the device, trigger secondary(subtasks) tasks |  |  | 25/11/2018 |
| H5 | Be able to use sliders | Interact with the device, navigate menu | C |  | 25/11/2018 |
| H6 | View feedback on screen | Ensure that button clicks are registered | C |  | 25/11/2018 |
| H7 | View feedback on LEDs | Ensure that button clicks are registered | C |  | 25/11/2018 |
| H8 | Enter user information | Have multiple user profiles | N |  | 25/11/2018 |
| H9 | Change scale of BPM using slider | View more precise readings | C |  | 25/11/2018 |
| H10 | Change the scale of the UI using the slider | I can enlarge the words on screen | N |  | 25/11/2018 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Screen (Huseyin Sert) | | | | | |
| S1 | Display blood pressure reading | See blood pressure reading | S |  | 25/11/2018 |
| S2 | Show other data being read from the device | The screen real estate is used effectively | N |  | 25/11/2018 |
| S3 | Display blood pressure reading in real time | Ensure that the device is working properly, Tell patient what is going on with their readings | S |  | 25/11/2018 |
| S4 | Display multiple blood pressure readings | Compare readings | N |  | 25/11/2018 |
| S5 | Display Menu | Select different menu option, Perform different tasks | S |  | 25/11/2018 |
| S6 | Display text and data in a clear and readable format | See text and data on the screen clearly | S |  | 25/11/2018 |
| S7 | Display message on boot-up | Indicate that the screen will be working | S |  | 25/11/2018 |

# **Acceptance Tests**

## **POST/Power On (Harrison James Marcks)**

**Test Name**: PP\_T1  
**Requirements Tested**: P1  
**Outline**: Ensure that the system tests the memory  
**Pre-requisites**: System is turned off  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Turn on the system | The system will start to display information to the screen |
| 2 | Wait | The system will eventually be started |

**Test Name**: PP\_T2  
**Requirements Tested**: P2  
**Outline**: Ensure that the system tests the screen  
**Pre-requisites**: System is turned off  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Turn on the system | The system will start to display characters on the screen |
| 2 | Wait | Eventually, it’ll move on to the next test |

**Test Name**: PP\_T3  
**Requirements Tested**: P3  
**Outline**: Ensure that the CPU instructions work correctly  
**Pre-requisites**: System is turned off  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Turn on the system | Diagnostic information will be displayed on the screen relating to the jump instructions being tested |
| 2 | Wait | Eventually the system will move onto the next test |

**Test Name**: PP\_T4  
**Requirements Tested**: P4  
**Outline**: Make sure the power is stable  
**Pre-requisites**: System is turned off  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Turn on the system | System shows it is starting |
| 2 | Wait | Information relating to the power supply is displayed |

**Test Name**: PP\_T5  
**Requirements Tested**: P5  
**Outline**: Test the ROM to make sure everything is okay  
**Pre-requisites**: System is turned off  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Turn on the system | System shows it is starting |
| 2 | Wait | System shows ROM diagnostic information on the screen |

**Test Name**: PP\_T6  
**Requirements Tested**: P6  
**Outline**: The POST/Power On tests should be able to run  
**Pre-requisites**: System is turned off  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Turn the system on | The first test is run |
| 2 | Wait | Each subsequent test is run one after another |
| 3 | Wait | All tests have been run and the system is in a sane state OR some diagnostic information is being displayed |

**Test Name**: PP\_T7  
**Requirements Tested**: P7  
**Outline**: Check to make sure the buttons can be read from  
**Pre-requisites**: System is turned off  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Turn on the system | The system shows it is starting |
| 2 | Ask for user input on both buttons | The system confirms each button press and carries on |

**Test Name**: PP\_T8  
**Requirements Tested**: P8  
**Outline**: Check network interface  
**Pre-requisites**: System is turned off  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Turn the system on | System shows it is starting |
| 2 | Wait | The system performs a Hardware check to see if there is an Ethernet or Wi-Fi  Module |

**Test Name**: PP\_T9  
**Requirements Tested**: P9  
**Outline**: Check blue-tooth module  
**Pre-requisites**: System is turned off  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Turn on the system | System shows it is starting |
| 2 | Wait | The system performs a Hardware check to see if there is a blue-tooth module installed |

**Test Name**: PP\_T10  
**Requirements Tested**: P10, P1, P2, P3, P4, P5, P6, P7, P8, P9   
**Outline**: Perform all tests in sequence at system boot  
**Pre-requisites**: System is turned off  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Turn on the system. | The system shows it has begun booting using the LEDs |
| 2 | Wait | Eventually the screen will begin to show POST diagnostic information |
| 3 | Wait | More tests will appear on the screen and completed one after another |
| 4 | Wait | Eventually a splash screen will be displayed, and the user will be informed of any tests that may have failed. |

## **Blood Pressure Machine (Huseyin Sert)**

**Test Name**: B\_T1  
**Requirements Tested**: B1, B2, B3, B6  
**Outline**: Ensure that the device can measure user’s blood pressure  
**Pre-requisites**: Make sure the device is turned on, healthy and sensors connected

**Method:**

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1. | Attach the sensors to a person | Sensors are properly attached to a person |
| 2. | Once the reading is completed, look at the blood pressure reading on the display | See a reasonable blood pressure reading |
| 3. | Repeat the above ***STEP***s again to check if readings are consistent | See same or very similar blood pressure readings |

**Test Name**: B\_T2  
**Requirements Tested**: B4  
**Outline**: Ensure that the device can take the average blood pressure  
**Pre-requisites**: Make sure the device is turned on, healthy and sensors connected

**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1. | Attach the sensors to a person | Sensors are properly attached to a person |
| 2. | Get three different readings from the machine in one sitting | End up with three very similar readings |
| 3. | Once the readings are completed, select the “average” option from the menu | Observe the “average” option returning the average result of the last three readings |

**Test Name**: B\_T3

**Requirements Tested**: B1, B2, B3, B4, B5, B6

**Outline**: Ensure that the device can filter out erroneous readings and data

**Pre-requisites**: Make sure the device is turned on, healthy and sensors connected  
**Method:**

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1. | Attach the sensors to a person | Sensors are properly attached to a person |
| 2. | Get different readings from the machine | See the readings on the screen |
| 3. | If some readings are unusually high or low due to – person: not resting 3-5 minutes, talking, has fluctuating body temperature, smoking cigarette less than 30 mins prior to reading or other reasons, identify these readings and delete them. | See a realistic and accurate readings |

## **Human Interface (Huseyin Sert)**

**Test Name**: HI\_T1  
**Requirements Tested**: H1. H2, H3, H4  
**Outline**: Ensure that a single button click is registered as only a click  
**Pre-requisites**: System is turned on, healthy, and ready to receive input  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Click the button for an option | No other type of button press is registered |

**Test Name**: HI\_T2  
**Requirements Tested**: H1. H2, H3, H4  
**Outline**: Ensure that a double button click is registered as only a double click  
**Pre-requisites**: System is turned on, healthy, and ready to receive input  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Double click an option | No other type of button press is registered |

**Test Name**: HI\_T3  
**Requirements Tested**: H1. H2, H3, H4  
**Outline**: Ensure that a single long press is registered as only a long a press  
**Pre-requisites**: System is turned on, healthy, and ready to receive input  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Hold button down to select an option | No other type of button press is registered |

**Test Name**: HI\_T4  
**Requirements Tested**: H1. H2, H3, H4  
**Outline**: Ensure that pressing multiple buttons at once is registered as nothing else  
**Pre-requisites**: System is turned on, healthy, and ready to receive input  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Push multiple buttons | No other type of button press is registered |

**Test Name**: HI\_T5  
**Requirements Tested**: H5  
**Outline**: Use the slider to change an option  
**Pre-requisites**: System is turned on, healthy, and ready to receive input  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Adjust the slider such that an option is changed | The slider input is correctly handled |

**Test Name**: HI\_T6  
**Requirements Tested**: H6  
**Outline**: View feedback on the screen  
**Pre-requisites**: System is turned on, healthy, and ready to send output  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Make changes to the system such that what is displayed to the user will change | Any changes or actions carried out by the user are communicated to them |

**Test Name**: HI\_T7  
**Requirements Tested**: H7  
**Outline**: View feedback on the LEDs  
**Pre-requisites**: System is turned on, healthy, and ready to send output  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Perform a button press | See LEDs response via quick blink, demonstrating that button click has been registered |

**Test Name**: HI\_T8  
**Requirements Tested**: H8  
**Outline**: Enter information on a user  
**Pre-requisites**: System is turned on, healthy, and ready to receive input  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Goto user profiles |  |
| 2 | Create or edit a new user |  |
| 3 | Enter user information using various combinations of the button presses | The data being entered can be entered by the user using the buttons |

**Test Name**: HI\_T9  
**Requirements Tested**: H9  
**Outline**: Use the slider to change the BPM scale  
**Pre-requisites**: System is turned on, healthy, and ready to receive input  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | Navigate to BPM screen option |  |
| 2 | Use the slider to zoom in/out | The readings are enlarged |

**Test Name**: HI\_T10  
**Requirements Tested**: H10  
**Outline**: Change the scale of the UI using the slider  
**Pre-requisites**: System is turned on, healthy, and ready to receive input  
**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1 | While on any screen use the slider to change the scale of the text and other things | The text is enlarged/shrunk |

## **Screen (Huseyin Sert)**

**Test Name**: S\_T1  
**Requirements Tested**: S1, S3   
**Outline**: Ensure that the screen displays the blood pressure reading  
**Pre-requisites**: Device is turned on, healthy and sensors are connected

**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1. | Wait for machine to take the reading | Machine is taking a reading |
| 2. | Once reading is complete, check the screen | See a blood pressure reading |

**Test Name**: S\_T2  
**Requirements Tested:** S2  
**Outline**: Ensure that the screen displays all the available / useful data  
**Pre-requisites:** Device is turned on and healthy

**Method:**

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1. | Connect all the sensors and peripherals that can be connected | All sensors and peripherals are fully connected |
| 2. | Make sure that all the data is formatted perfectly on the screen so that every useful and available data can displayed on one screen | View all the available / useful data in one screen without any data missing or protruding out of the screen |

**Test Name:** S\_T3  
**Requirements Tested:** S1, S3   
**Outline:** Ensure that the screen displays blood pressure reading in real time  
**Pre-requisites:** Device is turned on, healthy and sensors are connected  
**Method:**

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1. | Attach sensors to a person | Sensors are connected to a person |
| 2. | Wait for machine to take the reading | Machine is taking a reading |
| 3. | Look at the screen | See the reading values change as the reading is still in progress |

**Test Name**: S\_T4  
**Requirements Tested**: S4  
**Outline**: Ensure that the screen can show multiple blood pressure readings at the same time  
**Pre-requisites**: Device is turned on and healthy  
**Method:**

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1. | Navigate to where the user profiles are on the menu | See a list of users |
| 2. | Select a user from the list | See a list of previous readings on one screen |

**Test Name**: S\_T5  
**Requirements Tested**: S5   
**Outline**: Ensure that the screen can display a menu **Pre-requisites**: Device is turned on and healthy

**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1. | Look at the screen | See a list of options available to pick for different tasks |

**Test Name**: S\_T6  
**Requirements Tested**: S6  
**Outline**: Ensure that the screen can display text and data on the screen clearly with correct colour inversion **Pre-requisites**: Device is turned on and healthy

**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1. | Look at the screen | Be able to read text, options, menu and anything intended to be displayed on the screen without difficulty because a clear font is selected and correct colour inversion is being used |

**Test Name**: S\_T7  
**Requirements Tested**: S7  
**Outline**: Ensure that the screen can display a boot-up message **Pre-requisites**: Device is healthy

**Method**:

|  |  |  |
| --- | --- | --- |
| **STEP** | Action | Expected Observation |
| 1. | Boot the device up | See a small message on the screen before the device is fully booted |

# **Designs**

## **Screen**

### High Level (Huseyin Sert)

